<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<metadata><idinfo><citation><citeinfo><origin>U.S. Geological Survey (USGS) - Indiana Water Science Center (INWSC)</origin><pubdate>December of 2011</pubdate><title>elev_718_0, elev_718_5, elev_719_5, elev_720_5, elev_721_5, elev_722_5, elev_723_5, elev_724_5, elev_725_5, elev_726_5, elev_727_5, elev_728_5, elev_729_5, elev_730_5, elev_731_5, elev_732_5</title><geoform>vector digital data</geoform><onlink>NA</onlink></citeinfo></citation><descript><abstract>This vector file represents estimated extent of flooding based on modeled water surface elevations as determined for the White River near Nora, IN (USGS 03351000). This file contains the one of the following GIS layers: elev_718_0, elev_718_5, elev_719_5, elev_720_5, elev_721_5, elev_722_5, elev_723_5, elev_724_5, elev_725_5, elev_726_5, elev_727_5, elev_728_5, elev_729_5, elev_730_5, elev_731_5, elev_732_5. Additional information can be obtain from the following website: http://pubs.usgs.gov/sir/2011/5138/.</abstract><purpose>This data set was developed for use with the National Weather Service's (NWS) Advanced Hydrologic Prediction Service (AHPS) website (http://water.weather.gov/ahps/) and the U.S. Geological Survey Flood Inundation Mapping Science website (http://water.usgs.gov/osw/flood_inundation/).</purpose></descript><timeperd><timeinfo><sngdate><caldate>December of 2011</caldate></sngdate></timeinfo><current>ground condition</current></timeperd><status><progress>Complete.</progress><update>The data set will be maintained and updated as needed.</update></status><spdom><bounding><westbc>-86.146065</westbc><eastbc>-86.103807</eastbc><northbc>39.910368</northbc><southbc>39.869140</southbc></bounding></spdom><keywords><theme><themekt>flood, White River, Indiana, flood inundation mapping, hydrologic prediction, hydraulic, modeling</themekt><themekey>flood, White River, Indiana, flood inundation mapping, hydrologic prediction, hydraulic, modeling</themekey></theme></keywords><accconst>Free from restriction on use and distribution.</accconst><useconst>Users must assume responsibility to determine the appropriate use of this data. Users should be aware of the limitations of this dataset if using for critical application.</useconst><native>Microsoft Windows 2000 Version 5.2 (Build 3790) Service Pack 2; ESRI ArcCatalog 9.3.1.3000</native></idinfo><dataqual><attracc><attraccr>The attributes in this dataset are believed to be accurate.</attraccr></attracc><logic>These data are believed to be logically consistent, although not tested. Geometry appears topologically clean.</logic><complete>Spatial and attribute properties are believed to be complete, although attribute information has been simplified. No tests have been completed for exhaustiveness.</complete><posacc><horizpa><horizpar>Details of the process used to produce this data can be found in project documentation available from the data contact person. Horizontal accuracy was tested by evaluating boundaries to best available topographic dataset.</horizpar></horizpa><vertacc><vertaccr>Details of the process used to produce this data can be found in project documentation available from the data contact person. Vertical accuracy was tested by evaluating boundaries to best available topographic dataset.</vertaccr></vertacc></posacc><lineage><srcinfo><srccite><citeinfo><title>Observed and Forecast Flood-Inundation Mapping Application: A Pilot Study of an Eleven-Mile Reach of the White River, Indianapolis, Indiana; U.S. Geological Survey Scientific Investigations Report 2011–5138.</title><lworkcit><citeinfo><origin>U.S. Geological Survey (USGS) - Indiana Water Science Center (INWSC)</origin><title>Observed and Forecast Flood-Inundation Mapping Application: A Pilot Study of an Eleven-Mile Reach of the White River, Indianapolis, Indiana; U.S. Geological Survey Scientific Investigations Report 2011–5138.</title><onlink>http://pubs.usgs.gov/sir/2011/5138/</onlink></citeinfo></lworkcit></citeinfo></srccite><srcscale>U.S. Geological Survey (USGS) - Indiana Water Science Center (INWSC)</srcscale><typesrc>digital</typesrc><srccontr>The topographic data used for this work was obtained from existing digital elevation model contour datasets provided by the City of Indianapolis. The equivalent ground-elevation contour intervals of these data were two ft. throughout the study area.</srccontr></srcinfo><procstep><procdesc>USGS 2D hydraulic model (FaSTMECH) developed by the Geomorphology and Sediment Transport Laboratory was used to generate water surface elevations at one foot intervals above the near bank-full stage at White River near Nora, Indiana. The model also outputs depth information at each of the model nodes. Both water-surface elevation and water depth information are then converted to grid raster files with a cell size of 10 meters. Polygon vector files are then created from the grid raster files. The resulting polygons were edited to remove any flooding hydraulically disconnected from the main channel. Additional information can be obtain from the following website: http://pubs.usgs.gov/sir/2011/5138/.</procdesc><procdate>December of 2011</procdate><proctime>NA</proctime><srcprod>NA</srcprod></procstep><procstep><procdesc>Metadata imported.</procdesc><srcused>C:\DOCUME~1\mkim\LOCALS~1\Temp\xmlB3.tmp</srcused><procdate>20110823</procdate><proctime>16594300</proctime></procstep><procstep><procdesc Sync="TRUE">Dataset copied.</procdesc><srcused Sync="TRUE">\\sunset\StreamStats\flood_mapping_nws\fastmech_tmp\static2_50ft\nws_ahps\final_20110823\metadata_inundation_area_nora</srcused><procdate Sync="TRUE">20111209</procdate><proctime Sync="TRUE">15512600</proctime></procstep></lineage></dataqual><spdoinfo><direct>Vector</direct><ptvctinf><sdtsterm><sdtstype>G-polygon</sdtstype><ptvctcnt>1</ptvctcnt></sdtsterm></ptvctinf></spdoinfo><spref><horizsys><geograph><latres>0.000000</latres><longres>0.000000</longres><geogunit>Decimal degrees</geogunit></geograph><geodetic><horizdn>North American Datum of 1983</horizdn><ellips>Geodetic Reference System 80</ellips><semiaxis>6378137.000000</semiaxis><denflat>298.257222</denflat></geodetic></horizsys></spref><eainfo><detailed><enttyp><enttypl>elev_732_5</enttypl></enttyp><attr><attrlabl>FID</attrlabl><attrdef>Internal feature number.</attrdef><attrdefs>ESRI</attrdefs><attrdomv><udom>Sequential unique whole numbers that are automatically generated.</udom></attrdomv></attr><attr><attrlabl>Shape</attrlabl><attrdef>Feature geometry.</attrdef><attrdefs>ESRI</attrdefs><attrdomv><udom>Coordinates defining the features.</udom></attrdomv></attr><attr><attrlabl>Id</attrlabl></attr></detailed></eainfo><distinfo><resdesc>Downloadable Data</resdesc><stdorder><digform><digtinfo><transize>0.000</transize></digtinfo></digform></stdorder></distinfo><metainfo><metd>December of 2011</metd><metc><cntinfo><cntorgp><cntorg>U.S. Geological Survey (USGS) - Indiana Water Science Center (INWSC)</cntorg><cntper>Director</cntper></cntorgp><cntaddr><addrtype>5957 Lakeside Blvd.</addrtype><city>Indianapolis</city><state>Indiana</state><postal>46278</postal></cntaddr><cntvoice>317-290-3333</cntvoice></cntinfo></metc><metstdn>FGDC Content Standards for Digital Geospatial Metadata</metstdn><metstdv>FGDC-STD-001-1998</metstdv><mettc>local time</mettc><metextns><onlink>http://www.esri.com/metadata/esriprof80.html</onlink><metprof>ESRI Metadata Profile</metprof></metextns></metainfo><Esri><MetaID>{239F645C-29FF-4F51-9CA7-437E84A50CAA}</MetaID><CreaDate>20111209</CreaDate><CreaTime>15512600</CreaTime><SyncOnce>TRUE</SyncOnce></Esri><distInfo><distributor><distorTran><onLineSrc><linkage Sync="TRUE">file://\\sunset\StreamStats\flood_mapping_nws\fastmech_tmp\static2_50ft\nws_ahps\final_20111209\metadata_inundation_area_nora</linkage><protocol Sync="TRUE">Local Area Network</protocol></onLineSrc></distorTran></distributor></distInfo></metadata>